
**How to reboot telemetry board without shutting off AC to ETG transmitters**

1. Log into your WEB GUI interface.
2. Go to the “Wrench” icon on the top left of screen and select it. 
3. Go to the “Module Configuration” icon and select it.Graphical user interface

   Description automatically generated with medium confidence
4. Select the “Reboot” next to Reboot operating system. Graphical user interface

   Description automatically generated with medium confidence
5. This should reboot the telemetry card and should reconnect when finished.